**ROCKETBOX PRO MEASUREMENTS 2012**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Box | Length (in) | Width (in) | Height (in) | Capacity (ft^3) | Internal Length (lid support to lid support) (in) | Internal width (between the latches) (in) | Crossbar Spread minimum (in) | Crossbar Spread maximum (in) | Front Overhang Minimum (front lip to Xbar center) (in) | Front Overhang Maximum (front lip to Xbar center) (in) | Rear Overhang Minimum (rear lip to Xbar center)(in) | Rear Overhang Maximum (rear lip to Xbar center)(in) |
| RocketBox Pro 11 | 89 | 24 | 16 | 11.0 | 77.0 | 14.0 | 24 | 40 | 38 | 46 | 12.5 | 19 |
| RocketBox Pro 12 | 58 | 36 | 16 | 12.0 | 48.0 | 26.5 | 24 | 32 | 14 | 18 | 11 | 16 |
| RocketBox Pro 14 | 74 | 33 | 16 | 14.0 | 64.0 | 23.5 | 24 | 40 | 22 | 29.5 | 12 | 20 |

**SKYBOX MEASUREMENTS**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Box | Length (in) | Width (in) | Height (in) | Capacity (ft^3) | Internal Length (lid support to lid support) (in) | Internal width(between the latches) Min (in) | Crossbar Spread minimum (in) | CrossbarSpread maximum (in) | Front OverhangMinimum (front lip to Xbar center) (in) | Front OverhangMaximum (front lip to Xbar center) (in) | Rear OverhangMinimum (rear lip to Xbar center)(in) | Rear OverhangMaximum (rear lip to Xbar center)(in) |
| SKYBOX 12 | 92 | 24 | 16 | 12.0 | 80.0 | 18.5 | 24 | 42 | 25 | 33 | 24 | 32 |
| SKYBOX 16 | 81 | 36 | 15 | 16.0 | 70.0 | 29 | 24 | 36 | 21 | 27 | 22 | 28 |
| SKYBOX18 | 92 | 36 | 16 | 18.0 | 80.0 | 29 | 24 | 42 | 25 | 33 | 24 | 32 |
| SKYBOX21 | 92 | 36 | 18 | 21.0 | 80.0 | 29 | 24 | 42 | 25 | 33 | 24 | 32 |
| SKYBOX LOPRO | 92 | 36 | 11 | 15.0 | 80.0 | 29 | 24 | 42 | 25 | 33 | 24 | 32 |
| SkyBox NX 16 | 75.5 | 35 | 16 | 16.0 | 69.0 | 27 | 23.5 | 36 | 20.5 | 28.5 | 17 | 23 |
| SkyBox NX 18 | 84 | 36 | 16.5 | 18 | 77 | 27.5 | 23.5 | 40.25 | 23 | 32 | 19 | 28 |

 **GrandTour and CBX 2020**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Box | Length (in) | Width (in) | Height (in) | Capacity (ft^3) | Internal Length (lid support to lid support) (in) | Internal width(between the latches) Min (in) | Crossbar Spread minimum (in) | CrossbarSpread maximum (in) | Front OverhangMinimum (front lip to Xbar center) (in) | Front OverhangMaximum (front lip to Xbar center) (in) | Rear OverhangMinimum (rear lip to Xbar center)(in) | Rear OverhangMaximum (rear lip to Xbar center)(in) |
| GrandTour 16 | 79 | 35 | 17 | 16.0 | 74 |  26 | 24 | 36 | 19 | 25 | 21 | 30 |
| GrandTour 18 | 90555 | 37 | 16 | 18.0 | 85 | 27.5 | 24 | 40 | 19 | 32 | 19 | 27 |
| GrandTour LO | 90 | 37 | 10 | 15.0 | 85 | 27.5 | 24 | 40 | 19 | 37 | 19 | 27 |
| CBX 16/Solar | 83 | 38 | 15 | 16.0 | 77 | 29 | 24 | 34 | 17 | 36 | 17 | 20 |
| CBX 18 | 91 | 38 | 16 | 18.0 | 85 | 28.5 | 25 | 39 | 21 | 36 | 21 | 29 |

**RocketBox Pro METRIC**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Box | Length (cm) | Width (cm) | Height (cm) | Capacity (m^3) | Internal Length(lid support to lid support) (cm) | Internal width (between the latches) (cm) | Crossbar Spread minimum (cm) | CrossbarSpread maximum (cm) | Front OverhangMinimum (front lip to Xbar center) (cm) | Front OverhangMaximum (front lip to Xbar center) (cm) | Rear OverhangMinimum (rear lip to Xbar center) (cm) | Rear OverhangMaximum (rear lip to Xbar center) (cm) |
| RocketBox Pro 11 | 226 | 61 | 41 | 0.31 | 195.00 | 35.00 | 61 | 102 | 97 | 117 | 32 | 48 |
| RocketBox Pro 12 | 147 | 91 | 41 | 0.34 | 121.00 | 67.00 | 61 | 81 | 36 | 46 | 28 | 41 |
| RocketBox Pro 14 | 188 | 84 | 41 | 0.39 | 162.00 | 59.00 | 61 | 102 | 56 | 75 | 30 | 51 |

**SKYBOX METRIC**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Box | Length (cm) | Width (cm) | Height (cm) | Capacity (m^3) | Internal Length(lid support to lid support) (cm) | Internal width(between the latches) Min/Max (cm) | Crossbar Spread minimum (cm) | CrossbarSpread maximum (cm) | Front OverhangMinimum (front lip to Xbar center) (cm) | Front OverhangMaximum (front lip to Xbar center) (cm) | Rear OverhangMinimum (rear lip to Xbar center) (cm) | Rear OverhangMaximum (rear lip to Xbar center) (cm) |
| SKYBOX 12 | 234 | 61 | 41 | 0.34 | 203.0 | 39 /47 | 61 | 107 | 64 | 33 | 84 | 56 |
| SKYBOX 16 | 206 | 91 | 38 | 0.45 | 178.0 | 62 /74 | 61 | 91 | 53 | 27 | 56 | 71 |
| SKYBOX18 | 234 | 91 | 41 | 0.51 | 203.0 | 62 /74 | 61 | 107 | 64 | 33 | 84 | 56 |
| SKYBOX21 | 234 | 91 | 46 | 0.59 | 203.0 | 62 /74 | 61 | 107 | 64 | 33 | 84 | 56 |
| SKYBOX LOPRO | 234 | 91 | 28 | 0.42 | 203.0 | 62 /74 | 61 | 107 | 64 | 33 | 84 | 56 |